--- Power ---
VDD: B6 - Labeled 3V3, CN8, left side, 4th from top			VDD
GND: T6 - GND								GND

--- Timing ---
Interrupt_Monitor - CN11 left side, 1st from bot			PD9
Main_Monitor - CN12 right side, 1st from top				PC8

--- SPI ---
SPI3 CS: B1 - CN11, right side, 16th from top (next to A2)		PA4
SPI3 SCLK: B2 - CN11, left side, 1st from top				PC10
SPI3 MOSI: B3 - CN12, right side, 11th from top				PB2
SPI3 MISO: B4 - CN11, right side, 1st from top				PC11

--- User communication ---
ErrorCode_Bit_3 - CN12 right side, 4th from bot				PE0
ErrorCode_Bit_2 - CN12 right side, 3rd from bot				PG8
ErrorCode_Bit_1 - CN12 right side, 2nd from bot				PG5
ErrorCode_Bit_0 - CN12 right side, 1st from bot				PG6
LED_GREEN								PB0
LED_RED (Error detected - check bits 3-0)				PB14