Configuration	rhs_acquisition
STM32CubeMX 	6.18.0
Date	07/30/2026
MCU	STM32U5A5ZJTxQ



PERIPHERALS	MODES	FUNCTIONS	PINS
DEBUG	Trace Asynchronous Sw	DEBUG_JTMS-SWDIO	PA13 (JTMS/SWDIO)
DEBUG	Trace Asynchronous Sw	DEBUG_JTCK-SWCLK	PA14 (JTCK/SWCLK)
DEBUG	Trace Asynchronous Sw	DEBUG_JTDO-SWO	PB3 (JTDO/TRACESWO)
PWR:Low Power	Dead Battery Signals disabled	PWR_VS_DBSignals	VP_PWR_VS_DBSignals
PWR:Low Power	Power saving mode	PWR_VS_LPOM	VP_PWR_VS_LPOM
PWR:Security/Privilege attributes	Privilege attributes	PWR_VS_SECSignals	VP_PWR_VS_SECSignals
RCC	Crystal/Ceramic Resonator	RCC_OSC_IN	PH0-OSC_IN (PH0)
RCC	Crystal/Ceramic Resonator	RCC_OSC_OUT	PH1-OSC_OUT (PH1)
RCC	Crystal/Ceramic Resonator	RCC_OSC32_IN	PC14-OSC32_IN (PC14)
RCC	Crystal/Ceramic Resonator	RCC_OSC32_OUT	PC15-OSC32_OUT (PC15)
SPI1	Full-Duplex Master	SPI1_MISO	PA6
SPI1	Full-Duplex Master	SPI1_MOSI	PA7
SPI1	Full-Duplex Master	SPI1_SCK	PA1
SPI1	Hardware NSS Output Signal	SPI1_NSS	PA4
SYS	SysTick	SYS_VS_Systick	VP_SYS_VS_Systick
TIM3	Output Compare No Output	TIM3_VS_no_output1	VP_TIM3_VS_no_output1
USART1	Asynchronous	USART1_RX	PA10
USART1	Asynchronous	USART1_TX	PA9



Pin Nb	PINs	FUNCTIONs	LABELs
7	PC13	GPIO_EXTI13	
8	PC14-OSC32_IN (PC14)	RCC_OSC32_IN	
9	PC15-OSC32_OUT (PC15)	RCC_OSC32_OUT	
23	PH0-OSC_IN (PH0)	RCC_OSC_IN	
24	PH1-OSC_OUT (PH1)	RCC_OSC_OUT	
34	PA1	SPI1_SCK	
39	PA4	SPI1_NSS	
41	PA6	SPI1_MISO	
42	PA7	SPI1_MOSI	
75	PB14	GPIO_Input	UCPD_FLT
78	PD9	GPIO_Output	Interrupt_Monitor
87	PG2	GPIO_Output	LED_RED
90	PG5	GPIO_Output	ErrorCode_Bit_1
91	PG6	GPIO_Output	ErrorCode_Bit_0
93	PG8	GPIO_Output	ErrorCode_Bit_2
97	PC7	GPIO_Output	LED_GREEN
98	PC8	GPIO_Output	Main_Monitor
101	PA9	USART1_TX	
102	PA10	USART1_RX	
105	PA13 (JTMS/SWDIO)	DEBUG_JTMS-SWDIO	
109	PA14 (JTCK/SWCLK)	DEBUG_JTCK-SWCLK	
127	PG13	GPIO_Output	Compliance_Monitor
132	PB3 (JTDO/TRACESWO)	DEBUG_JTDO-SWO	
134	PB5	GPIO_Output	UCPD_DBn
136	PB7	GPIO_Output	LED_BLUE
140	PE0	GPIO_Output	ErrorCode_Bit_3
PERIPHERALS	MODES	FUNCTIONS	PINS
DEBUG	Trace Asynchronous Sw	DEBUG_JTMS-SWDIO	PA13 (JTMS/SWDIO)
DEBUG	Trace Asynchronous Sw	DEBUG_JTCK-SWCLK	PA14 (JTCK/SWCLK)
DEBUG	Trace Asynchronous Sw	DEBUG_JTDO-SWO	PB3 (JTDO/TRACESWO)
PWR:Low Power	Dead Battery Signals disabled	PWR_VS_DBSignals	VP_PWR_VS_DBSignals
PWR:Low Power	Power saving mode	PWR_VS_LPOM	VP_PWR_VS_LPOM
PWR:Security/Privilege attributes	Privilege attributes	PWR_VS_SECSignals	VP_PWR_VS_SECSignals
RCC	Crystal/Ceramic Resonator	RCC_OSC_IN	PH0-OSC_IN (PH0)
RCC	Crystal/Ceramic Resonator	RCC_OSC_OUT	PH1-OSC_OUT (PH1)
RCC	Crystal/Ceramic Resonator	RCC_OSC32_IN	PC14-OSC32_IN (PC14)
RCC	Crystal/Ceramic Resonator	RCC_OSC32_OUT	PC15-OSC32_OUT (PC15)
SPI1	Full-Duplex Master	SPI1_MISO	PA6
SPI1	Full-Duplex Master	SPI1_MOSI	PA7
SPI1	Full-Duplex Master	SPI1_SCK	PA1
SPI1	Hardware NSS Output Signal	SPI1_NSS	PA4
SYS	SysTick	SYS_VS_Systick	VP_SYS_VS_Systick
TIM3	Output Compare No Output	TIM3_VS_no_output1	VP_TIM3_VS_no_output1
USART1	Asynchronous	USART1_RX	PA10
USART1	Asynchronous	USART1_TX	PA9



Pin Nb	PINs	FUNCTIONs	LABELs
7	PC13	GPIO_EXTI13	
8	PC14-OSC32_IN (PC14)	RCC_OSC32_IN	
9	PC15-OSC32_OUT (PC15)	RCC_OSC32_OUT	
23	PH0-OSC_IN (PH0)	RCC_OSC_IN	
24	PH1-OSC_OUT (PH1)	RCC_OSC_OUT	
34	PA1	SPI1_SCK	
39	PA4	SPI1_NSS	
41	PA6	SPI1_MISO	
42	PA7	SPI1_MOSI	
75	PB14	GPIO_Input	UCPD_FLT
78	PD9	GPIO_Output	Interrupt_Monitor
87	PG2	GPIO_Output	LED_RED
90	PG5	GPIO_Output	ErrorCode_Bit_1
91	PG6	GPIO_Output	ErrorCode_Bit_0
93	PG8	GPIO_Output	ErrorCode_Bit_2
97	PC7	GPIO_Output	LED_GREEN
98	PC8	GPIO_Output	Main_Monitor
101	PA9	USART1_TX	
102	PA10	USART1_RX	
105	PA13 (JTMS/SWDIO)	DEBUG_JTMS-SWDIO	
109	PA14 (JTCK/SWCLK)	DEBUG_JTCK-SWCLK	
127	PG13	GPIO_Output	Compliance_Monitor
132	PB3 (JTDO/TRACESWO)	DEBUG_JTDO-SWO	
134	PB5	GPIO_Output	UCPD_DBn
136	PB7	GPIO_Output	LED_BLUE
140	PE0	GPIO_Output	ErrorCode_Bit_3



SOFTWARE PROJECT

Project Settings : 
Project Name : rhs_acquisition
Project Folder : C:\Users\afoy\Desktop\Software_Projects\STM32_Projects\U5_workspace\rhs_acquisition
Toolchain / IDE : STM32CubeIDE
Firmware Package Name and Version : STM32Cube FW_U5 V1.9.0


Code Generation Settings : 
STM32Cube MCU packages and embedded software packs : Copy only the necessary library files
Generate peripheral initialization as a pair of '.c/.h' files per peripheral : No
Backup previously generated files when re-generating : No
Delete previously generated files when not re-generated : Yes
Set all free pins as analog (to optimize the power consumption) : No


Toolchains Settings : 
Compiler Optimizations : 





