--- Power ---
VDD: B6 - Labeled 3V3, CN8, left side, 4th from top			VDD
GND: T6 - GND								GND

--- Timing ---
Interrupt_Monitor - CN11 left side, 1st from bot			PD9
Main_Monitor - CN12 right side, 1st from top				PC8
TIM1_ETR - CN12 right side, 14th from bot				PE7	wired to SPI3 CS - used to trigger timer pulse train ultimately used for 32-pulse SPI1 SCLK
TIM1_CH1 - CN12 right side, 10th from bot				PE9	wired to SPI1 SCLK - carries 32-pulse SPI1 SCLK

--- SPI ---
SPI3 CS: B1 - CN11, right side, 16th from top (next to A2)		PA4	wired to SPI1 CS
SPI1 CS: B1 - CN11, right side, 17th from top (next to A3)		PB0	wired to SPI3 CS
SPI3 SCLK: B2 - CN11, left side, 1st from top				PC10
SPI1 SCLK: CN11, right side, 15th from top (next to A1)			PA1	not connected to actual hardware, wired to TIM1_CH1 for internals
SPI3 MOSI: B3 - CN11, left side, 2nd from top				PC12
SPI3 MISO: B4 - CN11, right side, 1st from top				PC11	(only rhd_acquisition, wired to SPI1 MOSI - not used in rhd2164_acquisition)
SPI1 MOSI: B4 - CN12, left side, 8th from top				PA7	wired to SPI3 MISO

--- User communication ---
ErrorCode_Bit_3 - CN12 right side, 4th from bot				PE0
ErrorCode_Bit_2 - CN12 right side, 3rd from bot				PG8
ErrorCode_Bit_1 - CN12 right side, 2nd from bot				PG5
ErrorCode_Bit_0 - CN12 right side, 1st from bot				PG6
LED_GREEN								PC7
LED_RED (Error detected - check bits 3-0)				PG2